

 SAFE 2016 Post Tensioning 16.0.2 (Analysis Build 9548/32)
 File: C:\Users\ASUS\Desktop\Amir Kaviyani\SAFE\Safe.LOG




 B E G I N   A N A L Y S I S                                2018/02/06  10:01:47


 RUNNING ANALYSIS WITHIN THE GUI PROCESS
 USING THE ADVANCED SOLVER (PROVIDES LIMITED INSTABILITY INFORMATION)

 NUMBER OF JOINTS                          =        1408
    WITH RESTRAINTS                        =          16
 NUMBER OF FRAME/CABLE/TENDON ELEMENTS     =         424
 NUMBER OF SHELL ELEMENTS                  =        1136
 NUMBER OF LINK/SUPPORT ELEMENTS           =        4544
 NUMBER OF LOAD PATTERNS                   =           8
 NUMBER OF ACCELERATION LOADS              =           9
 NUMBER OF LOAD CASES                      =           9

 ADDRESSABLE PHYSICAL MEMORY (RAM)         =       2.000 GB

 PARALLELIZATION OF ANALYSIS OPERATIONS:
 (Env. variable SAPFIRE_NUM_THREADS        =           0)
 NUMBER OF THREADS: STATE (AUTOMATIC)      =           6
 NUMBER OF THREADS: STIFFNESS (AUTOMATIC)  =           6
 NUMBER OF THREADS: EVENT (AUTOMATIC)      =           6
 NUMBER OF THREADS: MOVE (AUTOMATIC)       =           6
 NUMBER OF THREADS: RESPONSE (AUTOMATIC)   =           6
 NUMBER OF THREADS: SOLVE (AUTOMATIC)      =           6


 E L E M E N T   F O R M A T I O N                                      10:01:47



 L I N E A R   E Q U A T I O N   S O L U T I O N                        10:01:47

 FORMING STIFFNESS AT ZERO (UNSTRESSED) INITIAL CONDITIONS

 TOTAL NUMBER OF EQUILIBRIUM EQUATIONS     =        4192
 NUMBER OF NON-ZERO STIFFNESS TERMS        =       53020

 ---------------------------------
 BASIC STABILITY CHECK FOR LINEAR LOAD CASES:
    NUMBER OF NEGATIVE STIFFNESS EIGENVALUES SHOULD BE ZERO FOR STABILITY.
    (NOTE: FURTHER CHECKS SHOULD BE CONSIDERED AS DEEMED NECESSARY,
     SUCH AS REVIEWING EIGEN MODES FOR MECHANISMS AND RIGID-BODY MOTION)

    NUMBER OF NEGATIVE EIGENVALUES         =           0,  OK.
 ---------------------------------


 L I N E A R   S T A T I C   C A S E S                                  10:01:47

 USING STIFFNESS AT ZERO (UNSTRESSED) INITIAL CONDITIONS

 TOTAL NUMBER OF CASES TO SOLVE            =           4
 NUMBER OF CASES TO SOLVE PER BLOCK        =           4

 LINEAR STATIC CASES TO BE SOLVED:

 CASE: DEAD
 CASE: LIVE
 CASE: EX
 CASE: EY


 N O N L I N E A R   S T A T I C   A N A L Y S I S                      10:01:47

 CASE: P01-NL

 STARTING FROM ZERO (UNSTRESSED) INITIAL CONDITIONS

 LOAD CONTROL TYPE                         =       FORCE
 TYPE OF GEOMETRIC NONLINEARITY            =        NONE
 INCLUDE ELASTIC MATERIAL NONLINEARITY     =          NO
 INCLUDE INELASTIC MATERIAL NONLINEARITY   =         YES
 USE EVENT STEPPING                        =         YES
 USE ITERATION                             =         YES
 USE LINE SEARCH                           =          NO
 EVENT LUMPING TOLERANCE                   =    0.010000
 FORCE CONVERGENCE TOLERANCE (RELATIVE)    =    1.00E-05

 Negative iterations are Constant-Stiffness
 Positive iterations are Newton-Raphson

  Saved    Null   Total  Iteration   Relative  Curr Step   Curr Sum    Max Sum
  Steps   Steps   Steps  this Step  Unbalance       Size   of Steps   of Steps
 (    1      25     200     -10/40   1.000000   1.000000   1.000000   1.000000)

      0       0       1  Conv   -1   1.52E-07   0.001000   0.001000   0.001000
      0       0       2  Conv   -1   0.000132   0.999000   1.000000   1.000000

 ----------------------------------------
 BASIC STABILITY CHECK FOR FORCE-CONTROLLED NONLINEAR STATIC LOAD CASES:
    NUMBER OF NEGATIVE STIFFNESS EIGENVALUES SHOULD BE ZERO FOR STABILITY.
    (NOTE: FURTHER CHECKS SHOULD BE CONSIDERED AS DEEMED NECESSARY)

    NUMBER FOUND AT FINAL CONVERGED STATE  =           0,  OK.
 ----------------------------------------

 NUMBER OF STIFFNESS FORMATIONS/SOLUTIONS  =           3

 TIME FOR INITIALIZING ANALYSIS            =        0.00
 TIME FOR CONTROLLING ANALYSIS             =        0.08
 TIME FOR UPDATING LOADS AND STATE         =        0.09
 TIME FOR FORMING STIFFNESS MATRIX         =        0.10
 TIME FOR SOLVING STIFFNESS MATRIX         =        0.17
 TIME FOR CALCULATING DISPLACEMENTS        =        0.07
 TIME FOR DETERMINING EVENTS               =        0.00
 TIME FOR SAVING RESULTS                   =        0.02
                                               ----------
 TOTAL TIME FOR THIS ANALYSIS              =        0.53


 N O N L I N E A R   S T A T I C   A N A L Y S I S                      10:01:48

 CASE: P02-NL

 STARTING FROM ZERO (UNSTRESSED) INITIAL CONDITIONS

 LOAD CONTROL TYPE                         =       FORCE
 TYPE OF GEOMETRIC NONLINEARITY            =        NONE
 INCLUDE ELASTIC MATERIAL NONLINEARITY     =          NO
 INCLUDE INELASTIC MATERIAL NONLINEARITY   =         YES
 USE EVENT STEPPING                        =         YES
 USE ITERATION                             =         YES
 USE LINE SEARCH                           =          NO
 EVENT LUMPING TOLERANCE                   =    0.010000
 FORCE CONVERGENCE TOLERANCE (RELATIVE)    =    1.00E-05

 Negative iterations are Constant-Stiffness
 Positive iterations are Newton-Raphson

  Saved    Null   Total  Iteration   Relative  Curr Step   Curr Sum    Max Sum
  Steps   Steps   Steps  this Step  Unbalance       Size   of Steps   of Steps
 (    1      25     200     -10/40   1.000000   1.000000   1.000000   1.000000)

      0       0       1  Conv   -1   4.44E-08   0.001000   0.001000   0.001000
      0       0       2  Conv   -1   4.86E-05   0.999000   1.000000   1.000000

 ----------------------------------------
 BASIC STABILITY CHECK FOR FORCE-CONTROLLED NONLINEAR STATIC LOAD CASES:
    NUMBER OF NEGATIVE STIFFNESS EIGENVALUES SHOULD BE ZERO FOR STABILITY.
    (NOTE: FURTHER CHECKS SHOULD BE CONSIDERED AS DEEMED NECESSARY)

    NUMBER FOUND AT FINAL CONVERGED STATE  =           0,  OK.
 ----------------------------------------

 NUMBER OF STIFFNESS FORMATIONS/SOLUTIONS  =           3

 TIME FOR INITIALIZING ANALYSIS            =        0.02
 TIME FOR CONTROLLING ANALYSIS             =        0.08
 TIME FOR UPDATING LOADS AND STATE         =        0.15
 TIME FOR FORMING STIFFNESS MATRIX         =        0.09
 TIME FOR SOLVING STIFFNESS MATRIX         =        0.15
 TIME FOR CALCULATING DISPLACEMENTS        =        0.06
 TIME FOR DETERMINING EVENTS               =        0.00
 TIME FOR SAVING RESULTS                   =        0.00
                                               ----------
 TOTAL TIME FOR THIS ANALYSIS              =        0.55


 N O N L I N E A R   S T A T I C   A N A L Y S I S                      10:01:48

 CASE: P03-NL

 STARTING FROM ZERO (UNSTRESSED) INITIAL CONDITIONS

 LOAD CONTROL TYPE                         =       FORCE
 TYPE OF GEOMETRIC NONLINEARITY            =        NONE
 INCLUDE ELASTIC MATERIAL NONLINEARITY     =          NO
 INCLUDE INELASTIC MATERIAL NONLINEARITY   =         YES
 USE EVENT STEPPING                        =         YES
 USE ITERATION                             =         YES
 USE LINE SEARCH                           =          NO
 EVENT LUMPING TOLERANCE                   =    0.010000
 FORCE CONVERGENCE TOLERANCE (RELATIVE)    =    1.00E-05

 Negative iterations are Constant-Stiffness
 Positive iterations are Newton-Raphson

  Saved    Null   Total  Iteration   Relative  Curr Step   Curr Sum    Max Sum
  Steps   Steps   Steps  this Step  Unbalance       Size   of Steps   of Steps
 (    1      25     200     -10/40   1.000000   1.000000   1.000000   1.000000)

      0       0       1  Conv   -1   4.32E-08   0.001000   0.001000   0.001000
      0       0       2  Conv   -1   4.21E-05   0.999000   1.000000   1.000000

 ----------------------------------------
 BASIC STABILITY CHECK FOR FORCE-CONTROLLED NONLINEAR STATIC LOAD CASES:
    NUMBER OF NEGATIVE STIFFNESS EIGENVALUES SHOULD BE ZERO FOR STABILITY.
    (NOTE: FURTHER CHECKS SHOULD BE CONSIDERED AS DEEMED NECESSARY)

    NUMBER FOUND AT FINAL CONVERGED STATE  =           0,  OK.
 ----------------------------------------

 NUMBER OF STIFFNESS FORMATIONS/SOLUTIONS  =           3

 TIME FOR INITIALIZING ANALYSIS            =        0.00
 TIME FOR CONTROLLING ANALYSIS             =        0.07
 TIME FOR UPDATING LOADS AND STATE         =        0.16
 TIME FOR FORMING STIFFNESS MATRIX         =        0.11
 TIME FOR SOLVING STIFFNESS MATRIX         =        0.16
 TIME FOR CALCULATING DISPLACEMENTS        =        0.06
 TIME FOR DETERMINING EVENTS               =        0.00
 TIME FOR SAVING RESULTS                   =        0.01
                                               ----------
 TOTAL TIME FOR THIS ANALYSIS              =        0.57


 N O N L I N E A R   S T A T I C   A N A L Y S I S                      10:01:49

 CASE: P04-NL

 STARTING FROM ZERO (UNSTRESSED) INITIAL CONDITIONS

 LOAD CONTROL TYPE                         =       FORCE
 TYPE OF GEOMETRIC NONLINEARITY            =        NONE
 INCLUDE ELASTIC MATERIAL NONLINEARITY     =          NO
 INCLUDE INELASTIC MATERIAL NONLINEARITY   =         YES
 USE EVENT STEPPING                        =         YES
 USE ITERATION                             =         YES
 USE LINE SEARCH                           =          NO
 EVENT LUMPING TOLERANCE                   =    0.010000
 FORCE CONVERGENCE TOLERANCE (RELATIVE)    =    1.00E-05

 Negative iterations are Constant-Stiffness
 Positive iterations are Newton-Raphson

  Saved    Null   Total  Iteration   Relative  Curr Step   Curr Sum    Max Sum
  Steps   Steps   Steps  this Step  Unbalance       Size   of Steps   of Steps
 (    1      25     200     -10/40   1.000000   1.000000   1.000000   1.000000)

      0       0       1  Conv   -1   1.13E-07   0.001000   0.001000   0.001000
      0       0       2  Conv   -1   0.000121   0.999000   1.000000   1.000000

 ----------------------------------------
 BASIC STABILITY CHECK FOR FORCE-CONTROLLED NONLINEAR STATIC LOAD CASES:
    NUMBER OF NEGATIVE STIFFNESS EIGENVALUES SHOULD BE ZERO FOR STABILITY.
    (NOTE: FURTHER CHECKS SHOULD BE CONSIDERED AS DEEMED NECESSARY)

    NUMBER FOUND AT FINAL CONVERGED STATE  =           0,  OK.
 ----------------------------------------

 NUMBER OF STIFFNESS FORMATIONS/SOLUTIONS  =           3

 TIME FOR INITIALIZING ANALYSIS            =        0.00
 TIME FOR CONTROLLING ANALYSIS             =        0.09
 TIME FOR UPDATING LOADS AND STATE         =        0.13
 TIME FOR FORMING STIFFNESS MATRIX         =        0.10
 TIME FOR SOLVING STIFFNESS MATRIX         =        0.16
 TIME FOR CALCULATING DISPLACEMENTS        =        0.06
 TIME FOR DETERMINING EVENTS               =        0.00
 TIME FOR SAVING RESULTS                   =        0.02
                                               ----------
 TOTAL TIME FOR THIS ANALYSIS              =        0.56


 N O N L I N E A R   S T A T I C   A N A L Y S I S                      10:01:50

 CASE: P05-NL

 STARTING FROM ZERO (UNSTRESSED) INITIAL CONDITIONS

 LOAD CONTROL TYPE                         =       FORCE
 TYPE OF GEOMETRIC NONLINEARITY            =        NONE
 INCLUDE ELASTIC MATERIAL NONLINEARITY     =          NO
 INCLUDE INELASTIC MATERIAL NONLINEARITY   =         YES
 USE EVENT STEPPING                        =         YES
 USE ITERATION                             =         YES
 USE LINE SEARCH                           =          NO
 EVENT LUMPING TOLERANCE                   =    0.010000
 FORCE CONVERGENCE TOLERANCE (RELATIVE)    =    1.00E-05

 Negative iterations are Constant-Stiffness
 Positive iterations are Newton-Raphson

  Saved    Null   Total  Iteration   Relative  Curr Step   Curr Sum    Max Sum
  Steps   Steps   Steps  this Step  Unbalance       Size   of Steps   of Steps
 (    1      25     200     -10/40   1.000000   1.000000   1.000000   1.000000)

      0       0       1  Conv   -1   1.26E-07   0.001000   0.001000   0.001000
      0       0       2  Conv   -1   0.000119   0.999000   1.000000   1.000000

 ----------------------------------------
 BASIC STABILITY CHECK FOR FORCE-CONTROLLED NONLINEAR STATIC LOAD CASES:
    NUMBER OF NEGATIVE STIFFNESS EIGENVALUES SHOULD BE ZERO FOR STABILITY.
    (NOTE: FURTHER CHECKS SHOULD BE CONSIDERED AS DEEMED NECESSARY)

    NUMBER FOUND AT FINAL CONVERGED STATE  =           0,  OK.
 ----------------------------------------

 NUMBER OF STIFFNESS FORMATIONS/SOLUTIONS  =           3

 TIME FOR INITIALIZING ANALYSIS            =        0.00
 TIME FOR CONTROLLING ANALYSIS             =        0.08
 TIME FOR UPDATING LOADS AND STATE         =        0.12
 TIME FOR FORMING STIFFNESS MATRIX         =        0.09
 TIME FOR SOLVING STIFFNESS MATRIX         =        0.15
 TIME FOR CALCULATING DISPLACEMENTS        =        0.07
 TIME FOR DETERMINING EVENTS               =        0.00
 TIME FOR SAVING RESULTS                   =        0.00
                                               ----------
 TOTAL TIME FOR THIS ANALYSIS              =        0.51


 A N A L Y S I S   C O M P L E T E                          2018/02/06  10:01:50
